CAUTION

**CONSULT OPERATING AND SERVICE MANUAL SECTION II BEFORE ATTEMPTING TO APPLY POWER. INTERNAL SHIPPING RESTRAINTS MUST BE REMOVED BEFORE APPLYING POWER OR DAMAGE TO THIS EQUIPMENT WILL RESULT.**

CUT PAPER TO 5.95” x 3.5”

106294-01