**Unlocking MOVCPM**

The new build **movpm** program might not work on your current system, DRI used a lot of serialization code in cpmove.asm to verify the kernel in movcpm.com with the current running one. The program will run into a HALT opcode which will abort the emulation, in case the versions don't match. To overcome this problem run **movcpm** under control of **ddt** and patch out the jumps to the error handler:

 ddt d:movcpm.com

 DDT VERS 2.2

 NEXT PC

 2700 0100

 -s234

 0234 C2 0

 0235 5A 0

 0236 02 0

 0237 02 .

 -s2cb

 02CB C2 0

 02CC 5A 0

 02CD 02 0

 02CE 23 .

 -i64 \*

 -g

 CONSTRUCTING 64k CP/M vers 2.2

 READY FOR "SYSGEN" OR

 "SAVE 34 CPM64.COM"